	Sonex-B
N830EH
	Maintenance Checklist
100-Hour Inspection



100-Hour Inspection Checklist
	Aircraft: N830EH
Make: Krueger Evan M
Model: Sonex B
Serial Number: 0849B
	Airframe TT: X.X
Engine Tach: X.X
Engine TT: X.X
Prop TT: X.XX
	Start Date: XX/XX/XXXX
End Date: XX/XX/XXXX
Performed By: Evan Krueger



Powerplant
	Inspection Item
	Fail
	Pass
	Comments

	Inspect engine compartment (pre-cleaning) 
[JEM0002-12 Section 8.8]
	
	
	

	Clean engine and engine compartment 
[JEM0002-12 Section 7.3]
	
	
	

	Inspect firewall for damage, cracks, proper sealant, and cleanliness
[JEM0002-12 Section 8.8]
	
	
	

	Inspect electrical wiring 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect starter and master solenoid connections 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect engine compartment including torque seal on through bolts
[JEM0002-12 Section 8.8]
	
	
	

	Inspect engine mounts and hardware for degradation and cracking
[JEM0002-12 Section 8.8]
	
	
	

	Inspect cylinders for oil leakage, cracks, discoloration, or damage
[JEM0002-12 Section 8.8]
	
	
	

	Inspect intake and exhaust system for damage and wear. 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect exhaust system springs and tabs
[AC43.13 Section 8-49]
	
	
	

	Inspect flywheel screws and check torque
[JEM0002-12 Section 9.23]
	
	
	

	Inspect crankcase and front seal for leaks
[JEM0002-12 Section 8.8]
	
	
	

	Inspect distributor caps & rotors and adjust as needed)
[JEM0002-12 Section 9.9]
	
	
	

	Inspect ignition coils, electrical connections, and coil gap
[JEM0002-12 Section 3.4]
	
	
	

	Inspect safety wires for condition and orientation
[AC43.13 Section 7-124]
	
	
	

	Inspect ram air ducts and baffles
[JEM0002-12 Section 8.8]
	
	
	

	Inspect engine controls and linkages for damage and smooth function
[JEM0002-12 Section 8.8]
	
	
	

	Perform fuel flow rate test and fuel shut off valve test
[JEM0002-12 Section 9.19]
	
	
	Fuel flow:

	Inspect fuel lines, fittings, and fire sleeves for condition and leaks
[AC43.13 Section 8-31]
	
	
	

	Inspect and replace fuel filter
[AC43.13 Section 8-36]
	
	
	

	Inspect air filter housing and replace air filter
[ACV-R10-01 Manual]
	
	
	

	Inspect AeroInjector for damage and rubber connector for cracking
[ACV-C07 Manual]
	
	
	

	Inspect oil hoses, lines, and fittings for condition and leaks
[AC43.13 Section 8-5]
	
	
	

	Check cylinder head bolt tension
[JEM0002-12 Section 9.15]
	
	
	

	Inspect top spring washer, valve springs, and rockers
[JEM0002-12 Section 9.16]
	
	
	

	Inspect hydraulic lifters and rockers
[JEM0002-12 Section 9.20]
	
	
	

	Perform pre-inspection test run
[JEM0002-12 Section 9.1]
	
	
	

	Change oil and oil filter 
[JEM0002-12 Section 9.5]
	
	
	

	Perform compression leak down check
[JEM0002-12 Section 9.18]
	
	
	#1:   /80 | #2:   /80 | #3:   /80 | #4:   /80 | #5:   /80 | #6:   /80

	Replace spark plugs and adjust gaps
[JEM0002-12 Section 3.4]
	
	
	

	Measure fluid in oil separator and empty 
[ACV-S03-01 Manual]
	
	
	Fluid Drained:





[bookmark: _Hlk212463940]Propeller
	Inspection Item
	Fail
	Pass
	Comments

	Inspect spinner for damage
[JEM0002-12 Section 8.7]
	
	
	

	Inspect propeller for damage, nicks, and corrosion
[JEM0002-12 Section 8.7]
	
	
	

	Check propeller bolts for proper torque
[JEM0002-12 Section 8.7]
	
	
	

	Perform propeller and spinner tracking procedures
[JEM0002-12 Section 9.2]
	
	
	



Airframe
	Inspection Item
	Fail
	Pass
	Comments

	Inspect welded components for cracks
[SNX-SB-002]
	
	
	




	Signature and Certificate #
	
	Date
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