	Sonex-B
N830EH
	Maintenance Checklist
25-Hour Inspection



25-Hour Inspection Checklist
	Aircraft: N830EH
Make: Krueger Evan M
Model: Sonex B
Serial Number: 0849B
	Airframe TT: X.X
Engine Tach: X.X
Engine TT: X.X
Prop TT: X.XX
	Start Date: XX/XX/XXXX
End Date: XX/XX/XXXX
Performed By: Evan Krueger



Powerplant
	Inspection Item
	Fail
	Pass
	Comments

	Inspect engine compartment (pre-cleaning) 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect intake and exhaust system for damage and wear. Verify cap screw torque 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect electrical wiring 
[JEM0002-12 Section 8.8]
	
	
	

	Inspect starter and master solenoid connections 
[JEM0002-12 Section 8.8]
	
	
	

	Measure fluid in oil separator and empty 
[ACV-S03-01 Manual]
	
	
	Fluid Drained:

	Change oil and oil filter 
[JEM0002-12 Section 9.5]
	
	
	

	Inspect top spring washer, valve springs, and rockers
[JEM0002-12 Section 9.16]
	
	
	



Airframe
	Inspection Item
	Fail
	Pass
	Comments

	Inspect welded components for cracks
[SNX-SB-002]
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